Time Shift (Actions)

The information is relevant for version 2.9.34 and later.

Description of Time Shift Actions.

Set video stream

Switching the signal source or file source to the module input.

Parameters

Param1 - input stream type.

FILE - file source.

LIVE - signal from the software module.

Param2 - file name, software module name.

Set format conversion

Sets the video conversion mode upon a mismatch of the input signal Aspect Ratio and the module settings.

Parameters

Param1 - conversion mode. Possible values: scale, crop, box, letter.

Param2 - AFD use flag. Possible values: true or false.

Set Source

Assigns a signal source for the service, with an option to select a different module’s output.

Parameters

Param1 - string with a new signal source. The string is specified in the format: shm_pal://SERVICE. For example: shm_pal://Capture_1