Replay Server Management from JavaScript via Instant Replay API

This page demonstrates possibilities of Skylark Instant Replay API.
To manage the replay server, open this page in a browser within one network with the replay server. The server must have access permission by the 10042 port for the XML-RPC protocol.

Server IP (necessarily) – your server IP address. To apply, press Set IP.

Clip Name (optional) – name of the clip (including multi-cam) in the server database that must be loaded to the replay server tray. For loading, press Load.

Slow Motion and Instant Replay Servers SL NEO 7000